Bumblebee Tutorial

Notes & Comments

Pulse Rate Frequency PRF (typical): 2 or 3 Mhz (500 or 333 nano sec interval)

Each pulse: 20 ns radio on; 15 ns radio off; 20 ns radio on; then off for rest of interval

At 2 MhZ, (20+15+20) / 500 = 11%

(Ananth): Fig 3. Note that the signals are not added but rather multiplied so that -2 \* -2 = +4.